**SWITCH MOLD INSERT QUOTE REQUEST**

**Inserts are available in 12mm, 14mm and 20mm diameters, see below for more information on available data specifications for each diameter.**

1. **Insert Dia:** **Quantity** **URL/DATA**
2. **Insert Dia:       Quantity       URL/DATA**
3. **Insert Dia:       Quantity       URL/DATA**

**Customer Account #** **Customer Address**

**Company Name** **Contact Name** **Phone or Email**

**\*\*For logos we will require dfx data file to be sent in**

**Specification & Examples of QR Code & Engraved Identifiers Mold Switch Inserts**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Insert Diameter** | **12 mm** | **12mm** | **12mm** | **12mm** |
| **CODE TYPE** | **Data Matrix** | **QR CODE** | **QR CODE** | **ENGRAVED IDENTIFIERS** |
| **Content Examples** | **DME Mold Component** | <https://www.dme.net/mdi> | https://www.dme. net/catalog/DME/ Mold%20Components/index.html#204 |  |
| **Max. numeric capacity** | **36** | **41** | **41** | **6** |
| **Max. alphanumeric capacity** | **25** | **25** | **25** | **6** |
| **Max. binary capacity** | **16** | **17** | **17** |  |
| **Error correcting rate** | **25%** | **7%** | **7%** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Insert Diameter** | **14mm** | **14mm** | **14mm** | **14 mm** |
| **CODE TYPE** | **Data Matrix** | **QR CODE** | **QR CODE** | **ENGRAVED IDENTIFIERS** |
| **Content Examples** | **DME Mold Component** | <https://www.dme.net/mdi> | https://www.dme. net/catalog/DME/ Mold%20Components/index.html#204 |  |
| **Max. numeric capacity** | **72** | **77** | **77** | **6** |
| **Max. alphanumeric capacity** | **52** | **47** | **47** | **6** |
| **Max. binary capacity** | **34** | **32** | **32** |  |
| **Error correcting rate** | **25%** | **7%** | **7%** |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Insert Diameter** | **20 mm** | **20mm** | **20mm** | **20 mm** |
| **CODE TYPE** | **Data Matrix** | **QR CODE** | **QR CODE** | **ENGRAVED IDENTIFIERS** |
| **Content Examples** | **DME Mold Component** | <https://www.dme.net/mdi> | https://www.dme. net/catalog/DME/ Mold%20Components/index.html#204 |  |
| **Max. numeric capacity** | **36** | **187** | **187** | **6** |
| **Max. alphanumeric capacity** | **25** | **114** | **114** | **6** |
| **Max. binary capacity** | **16** | **78** | **78** |  |
| **Error correcting rate** | **20-25%** | **8%** | **8%** |  |

**Return to** [**cs\_specials@dme.net**](mailto:cs_specials@dme.net) **or Call 1-800-626-6653 or (248) 398-6000**